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SGI030/035
Sensor head




Specifications
	Model
	SGI030/035

	Reference distance (RF)
	30mm

	Measuring range
	-5mm-5mm

	Light source
	Light source wavelength
	655nm

	
	Laser class
	Class II

	
	Laser output power
	5mW

	Laser point diameter (Light dot size)
	Small laser point
	Φ60μm

	
	Wide laser point
	60*400μm

	Repeatability①
	0.05um

	Linearity
	±0.05% F.S.

	Temperature characteristics
	0.01% F.S./℃

	Sampling refresh rate (Hz)
	1/2/5/10/20/50/88kHz (Choose from 7 levels)

	I/O
	Communication port
	1 100Base-TX/1000Base-T Ethernet interface, 1 RS485

	
	Analog output
	1-channel analog outputs, supports analog voltage and analog current switching

	
	IO input
	2 channels, timing, zeroing and single-ended encoder function multiplexing.

	
	IO output
	4 channel, determines status of output.

	Operating temperature
	0-50oC

	Storage temperature
	-20-70oC

	Working humidity
	35%-85% no condensation

	ESD protection
	Contact discharge 4kV, air discharge 8kV, conforms with IEC61000-4-2 standard

	EFT protection
	Power port 2kV/5 or 100kHz, signal port 1kV/5 or 100kHz, conforms with IEC61000-4-4

	Bumps
	50Gs/3ms on each axis, conforms with IEC 68-2-27 Ea

	Vibrations
	10Gs (10-500Hz), conforms with IEC 68-2-6 Fc

	IP level
	IP67, conforms with IEC 60529 standard

	Dimensions (mm)
	90x75x41

	Data cable (wiring) model
	SCB-GICAM-HA1-3m/6m/10m

	Weight (Including cables)
	324g


Note: ① Obtained from 4096 tests at reference distance.
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